|  |  |
| --- | --- |
| Author | Rizal Sharif |
| Name | System Issues |
| Title | APE New System |
| Date | 30.04.2015 |

|  |  |
| --- | --- |
| **Job Sheet - Repro**  **Barcode colour column:**   * The value does not appeared in the Job Sheet printout. |  |
| **Order Confirmation print out**  - Please included revision no. in the OC printout for Revision R1 and above  - Customer would like to differentiate between normal OC and Revision Job OC.  **Engraving Protocol – EMG**  Root Job no. not appeared in the print out.  **Remark:**  Root job no. also not appeared in **DLS protocol printout**.  Job Coordinator is missing. It should take the value from Job Coordinator field in Job Entry screen  Please follow the structure similar to input data in remark column  i.e. in 2 lines instead of 1 line.  It should be:  Line1: CMYK user JTI Gradation  Line2: Repro size:700mmx 512.76    **EMG Input screen**  Cell depth calculation is correct = 38.41452 . But once entered, the value will become CH value i.e 215.00000.  Please correct the value and make Cell Depth value without any decimal point.  Example 38.41452 = 38 | Wrong figure. Please correct the formula and make it without decimal value. |
| **Laser Etching Protocol.**  All the values cannot be changed. Once we change the value and saved it, the value will revert to the old value.  E.g. Job Order 1504/00556. |  |